Hi Eric, the values with a (T) are from Thierry and allright. For L3 from the Pitch Board I used 100 microHenry and for L2 10 microHenry. To get 6 mA from the current source I had to use 1k8 kOhm for R25 and R26. C28 =33pF(T). C35=470nF(T) Waveshaping: C17=10nF(T) C5=2,2nF(T). C11=100nF(T). VCF: C34, C31= 1nF(T). At first I used 820 pF and that did worked also good. Volume Board; all values are estimations: L1=47 uH, L2=22 uH C9=1500 pF C14=330 pF C15=6,8-10 nF C23=33pF C21= 470 nF- 1 uF Vol. CV processor: C3= 1nF C4= 100 nF C8= 10 nF I used that value because there is cap. of 10 nF between pin 6 and 7 of U 10-B seen on the photo of the Volume board not in the schematic! C12= 4,7 uF C22, C29 = 100 nF C31= 1 uF (seen on the photo!). C30, C32 not used. Pitch to CV converter not built, I use the P to V converter from the Etherwave Plus which I built earlier and besides I couldn’t get a MAT 04 anymore. Still this converters are much alike. Hope this will help. Henk

Pitch coil is 36 mH and Volume coil is 15 mH. Somewhat too high but thats not a big problem it is easy to retune because I use 2 200 microhenry coils in parallel and by bending these two coils from each other you can easily get everything right
